The model of the 14-generator power system introduced here is loosely based on the southern and eastern Australian networks. This test system can be used as a test bed for the small-signal analysis and design of power system stabilizers (PSSs) and other controllers *in a multi-machine power system*. Six difference cases with different load levels and unit dispatch plans are given.